				
			MCS9865 FREEBSD 6.4 Parallel port driver


Procedure:

	1. #make 	: To compile the driver.
	2. #make ld	: To load the driver.
	3. #make uld	: To unload the driver.


	After loading the driver, with dmesg command one should see the following messge.
The port names are /dev/lpt0 Use these names for accessing the ports.
 

ppc1: <NetMos NM9865 1284 Printer port> port 0xe800-0xe807,0xe480-0xe487 mem 0xfebfb000-0xfebfbfff,0xfebfa000-0xfebfafff irq 18 at device 0.2 on pci5
ppc1: Generic chipset (EPP/NIBBLE) in COMPATIBLE mode
ppbus3: <Parallel port bus> on ppc1


Usage:

Tested only command line printing.

	1. create a text file.
	2. print it using "cat <file name> > /dev/lpt0"
	

