CECInfo
(
	Name ( "MCS9865Ce50" )
	CECVersion ( 5.00 )
	GUID ( {87A50828-81DD-4EFE-89FB-49D6948C8573} )
)
ComponentType
(
	Name ( "MOSCHIP SEMICONDUCTOR PVT LTD-9865" )
	GUID ( {712FA09A-F629-4EE0-99D4-4F12C18CF5EE} )
	Description ( "PCI to Serial and Parallel Drivers" )
	Group ( "\Device Drivers" )
	MaxResolvedImpsAllowed( 999 )
	Implementations
	(
		Implementation
		(
			Name ( "Moschip PCI to Serial and Parallel Drivers(9865)" )
			GUID ( {9DCC82CA-0780-44EB-A679-B806E6E4CA8D} )
			Description ( "PCI to Serial and Parallel Drivers" )
			Version ( "1.0.0.2" )
			Locale ( 0409 )
			Vendor ( "Moschip Semiconductor Pvt Ltd" )
			Date ( "2/23/2009" )
			SizeIsCPUDependent( 1 )
			BuildMethods
			(
				BuildMethod
				(
					GUID ( {CDE12DF2-F12F-4B18-B3A7-19A300831400} )
					Step ( CESYSGEN )
					CPU ( "x86" )
					Action ( '#SRCCODE( USER_PROJECT, "$(_WINCEROOT)\PLATFORM\MCS9865Ce50\MCS9865Ce50.pbpxml" )' )
				)
			)
		)
	)
)
