Procedure for installing serial application(minicom)

1. cd MCS9865_VX.xx.xx
2. cd serialapp
3. pkg_add lrzsz-0.12.20_1.tbz
4. pkg_add minicom-2.3_1.tbz


Procedure for kernel compilation.

1. Install the kernel source
2. cd /usr/src/sys/i386/conf
3. cp GENERIC MYKERNEL
4. vi MYKERNEL ( edit MYKERNEL and add following lines in the file)

	a)Serial port section which is defined as Serial

	#Serial(COM) ports
	options	COM_MULTIPORT
	device		sio
	device		uart

	b)Parallel port section which is defined as parallel port

	#parallel port
	#device		ppc	#disable built-in parallel port support

	c)Dumb serial and parallel port section
	
	device		puc	#enable puc support


5.  config MYKERNEL
6.  cd ../compile/MYKERNEL
7.  make cleandepend
8.  make depend
9.  make
10. make install
11. reboot
